Cisco Packet Tracer Version: 7.3.0.0838

**Documentation:**

At first, made the full VLSM table.  
Then, at router0 set a pc as console and by the pc enter to the terminal(the console of router 0).

Then enter the command to set my name as the hostname of router 0:

1.enable

2.configure terminal

3.hostname Niamul

Then configure the routers (version 2 routing protocol) and servers (using sequential IPs).

configure the DNS server.

Set PC’s at BBA and CSE.  
Check everything is ok or not .!

done..!